mode locking method

There are many ways to generate ultrafast laser operations. One can use real saturable absorbers, such as semiconductor saturable absorber mirror (SEASM) [SESAM mode-locked red praseodymium laser] or low-dimensional material-based saturable absorbers such as graphene [] and blablabla [], and solid-state laser media []. One can also exploit artificial saturable absorbers. The two most prominent artificial saturable absorber mode locking techniques are called Kerr-Lens Mode Locking (KLM) [1][2][3][4][5][6][7] early[8][9][10] and Additive Pulse Mode Locking (APM) [].

Pr:YLF

By virtue of its vast variety of robust emission lines ranging from visible to near infrared spectral range, trivalent praseodymium (Pr3+) ions have been identified as one of the most potential candidates for efficient visible lasers.

In recent years, with the development of blue laser diodes (LDs), which are both compact and easily available, diode-pumped all solid-state Pr3+-doped material visible lasers are gradually attracting more and more attention.

CW

In the field of continuous-wave (cw) visible laser operations, enormous progresses have been achieved with Pr3+-doped materials, such as LiYF4 waveguide [Red and orange Pr3+:LiYF4 planar waveguide laser, Green, orange, and red Pr3+∶YLiF4 epitaxial waveguide lasers], ZBLAN fiber [Blue Pr3+-doped ZBLAN fiber upconversion laser, Visible–NIR tunable Pr3+-doped fiber laser pumped by a GaN laser diode], waterproof fluoroaluminate glass fiber [High-power direct green laser oscillation of 598 mW in Pr3+-doped waterproof fluoroaluminate glass fiber excited by two-polarization-combined GaN laser diodes] or LiLuF4 monocrystalline fiber [Visible laser operation in a Pr3+:LiLuF4 monocrystalline fiber grown by the micro-pulling-down method] and crystals such as LiYF4 [Diode pumping of a continuous-wave Pr3+-doped LiYF4 laser], LiLuF4 [Visible laser emission of solid state pumped LiLuF4:Pr3+], LaF3 [Diode pumped laser operation and spectroscopy of Pr3+:LaF3] and KY3F10[Wide wavelength tunability and green laser operation of diode-pumped Pr3+:KY3F10]. Lately, cw watt-level high power Pr:YLF visible lasers pumped by intra-cavity frequency-doubled Optically Pumped InGaAs Semiconductor Laser (2ω-OPSL) [High-power red, orange, and green Pr3+:LiYF4 lasers] or LD [Power scaling of blue-diode-pumped Pr:YLF lasers at 523.0, 604.1, 606.9, 639.4, 697.8 and 720.9nm] have been realized with high efficiencies.

Q switching

Regarding the pulsed oscillation of LD-pumped Q-switched Pr3+ ion lasers with kilohertz repetition rates and nanosecond pulse widths,

actively [Intracavity second-harmonic generation at 320 nm of an actively Q-switched Pr:LiYF4 laser, InGaN diode pumped actively Q-switched intracavity frequency doubling Pr:LiYF4 261 nm laser]

passive Q-switching was reported with a semiconductor saturable absorber mirror (SESAM) [2011 Passively Q-switched Pr:YLF laser],

[2012 Wavelength Tunable Q-switch Laser in Visible Region with Pr3+-doped Fluoride-glass Fiber Pumped by GaN Diode Lasers] We report passively Q-switched operation of a diode-pumped Pr:YLF laser using an AlInGaP on GaAs SEmiconductor Saturable Absorber Mirror. Q-switched pulses with 145ns duration and 23mW average output power at 639.5nm are obtained.

Cr4+:YAG crystal [Cr4+-Doped Y3Al5O12 as a Saturable Absorber for a Q-Switched and Mode-Locked 639-nm Pr3+-Doped LiYF4 Laser, Saturation of 640-nm absorption in Cr4+:YAG for an InGaN laser diode pumped passively Q-switched Pr3+:YLF laser, 50-kHz, 50-ns UV pulse generation by diode-pumped frequency doubling Pr3+:YLF Q-switch laser with a Cr4+:YAG saturable absorber], gold nanoparticles [Gold nanoparticles as a saturable absorber for visible 635 nm Q-switched pulse generation], and nanosheets of transition metal dichalcogenides (TMDs) [Atomic-layer molybdenum sulfide optical modulator for visible coherent light, Passive Q-switching of a diode-pumped Pr:LiYF4 visible laser using WS2 as saturable absorber] as saturable absorbers.

mode locking

As for mode locking operations, The first mode-locked Pr3+:YLiF4 visible lasers at 607 and 640 nm utilizing the Kerr-lensing effect and initiated by saturable absorbers were realized in 1995 by introducing argon-ion lasers as the pump source. [Kerr-lens mode-locked visible transitions of a Pr:YLF laser]. The first self-staring Kerr-lens mode locked laser at 607 nm with pulses width of 15 ps was reported in 1996, which was also pumped by an argon-ion laser [Self-starting Kerr-lens mode-locked femtosecond Cr4+:YAG and picosecond Pr3+:YLF solid-state lasers]. In 2014, pumped by an 2ω-OPSL, the first semiconductor saturable absorber mirror (SESAM) mode-locked praseodymium solid-state laser at 640 nm was obtained by Gaponenko et al, with pulses duration of ∼18 ps. [SESAM mode-locked red praseodymium laser]. Due to the narrow gain bandwidth of the transition (3P0→3F2) in the Pr3+:YLF, generating mode-locked sub-picosecond pulses is challenging. The maximum averaged output power reached 16 mW at an incident pump power of 3.75 W.

In the past one year, the wavelength of self-mode-locked visible pulsed lasers extent to the spectral range of green and deep red for the first time [Laser-diode pumped self-mode-locked praseodymium visible lasers with multi-gigahertz repetition rate]. The system was pumped by laser-diode and the repetition rates were multi-gigahertz (GHz). The maximum output power reached 612 mW with the slope efficiency of 46.9% at 639 nm. Following closely, still by introducing a SESAM, but pumped by InGaN laser-diode, which is different from Gaponenko et al, mode-locking operation at the wavelength of 640 nm was attained. [Pr3+:YLF mode-locked laser at 640 nm directly pumped by InGaN-diode lasers]. a maximum averaged output power of 65 mW was obtained at absorbed pump power of 3.8 W, with a pulse width of 45 ps (FWHM) at a pulse repetition rate of 108 MHz.

**References**

[Nonlinear refractive indices of disordered NaT(XO4)2 T=Y, La, Gd, Lu and Bi, X=Mo, W femtosecond laser crystals]. A. García-Cortés, M. D. Serrano, C. Zaldo, C. Cascales, G. Strömqvist, and V. Pasiskevicius, “Nonlinear refractive indices of disordered NaT(XO4)2 T=Y, La, Gd, Lu and Bi, X=Mo, W femtosecond laser crystals,” Appl. Phys. B 91, 507-510 (2008).

[Novel self-mode-locking mechanism in narrow-band lasers]. Y. Bai, S. Chen, Z. Wang, and G. Zhang, Appl. Phys. Lett. 63, 2597 (1993).

[SESAM mode locked red praseodymium laser]. M. Gaponenko, P. W. Metz, A. Härkönen, A. Heuer, T. Leinonen, M. Guina, T. Südmeyer, G. Huber, and C. Kränkel, “SESAM modelocked red praseodymium laser,” Opt. Lett. 39, 6939–6941 (2014).

[Red-luminescence analysis of Pr3+ doped fluoride crystals] S. Khiari, M. Velazquez, R. Moncorge, J.L. Doualan, P. Camy, A. Ferrier, M. Diaf, J. Alloys Compd. 451 (2008) 128–131

[Pump-to-mode size ratio dependence of thermal loading in diode-end-pumped solid-state lasers]. Y. F. Chen, “Pump-to-mode size ratio dependence of thermal loading in diode-end-pumped solid-state lasers,” J. Opt. Soc. Am. B 17(2000) 1835.

[Theory of passive additive-pulse mode locking].

[Additive pulse mode locking]. E. P. Ippen, H. A. Haus, and L. Y Liu, “Additive pulse mode locking,” J. Opt. Soc. Am. B 6, 1736 (1989).

[SESAM mode-locked red praseodymium laser]. Maxim Gaponenko, Philip Werner Metz, Antti Härkönen, Alexander Heuer, Tomi Leinonen, Mircea Guina, Thomas Südmeyer, Günter Huber, and Christian Kränkel, “SESAM mode-locked red praseodymium laser,” Opt. Lett. 39(24), 6939 (2014)

[Kerr-lens mode-locked visible transitions of a Pr:YLF laser]. S. Ruan, B. H. T. Chai, J. M. Sutherland, P. M. W. French, and J. R. Taylor, “Kerr-lens mode-locked visible transitions of a Pr:YLF laser,” Opt. Lett. 20, 1041–1043 (1995).

[Self-starting Kerr-lens mode-locked femtosecond Cr4+:YAG and picosecond Pr3+:YLF solid-state lasers]. Y. P. Tong, A. V. Shestakov, B. H. T. Chai, J. M. Sutherland, P. M. W. French, and J. R. Taylor, “Self-starting Kerr-lens mode-locked femtosecond Cr4+:YAG and picosecond Pr3+:YLF solid-state lasers,” Opt. Lett. 21, 644–646 (1996).

[Pr3+:YLF mode-locked laser at 640 nm directly pumped by InGaN-diode lasers]. KODAI IIJIMA, RYOSUKE KARIYAMA, HIROKI TANAKA, AND FUMIHIKO KANNARI, “Pr3+:YLF mode-locked laser at 640 nm directly pumped by InGaN-diode lasers,” Appl. Opt. 55(28), 7782 (2016)

[Laser-diode pumped self-mode-locked praseodymium visible lasers with multi-gigahertz repetition rate]. YUXIA ZHANG, HAOHAI YU, HUAIJIN ZHANG, ALBERTO DI LIETO, MAURO TONELLI, AND JIYANG WANG, “Laser-diode pumped self-mode-locked praseodymium visible lasers with multi-gigahertz repetition rate,” Opt. Lett. 41(12), 2692(2016)

[High-power red, orange, and green Pr3+:LiYF4 lasers]. Philip Werner Metz, Fabian Reichert, Francesca Moglia, Sebastian Müller, Daniel-Timo Marzahl, Christian Kränkel, and Günter Huber, “High-power red, orange, and green Pr3+:LiYF4 lasers.” Opt. Lett. 39(11), 3193(2014)

[Power scaling of blue-diode-pumped Pr:YLF lasers at 523.0, 604.1, 606.9, 639.4, 697.8 and 720.9nm]. Saiyu Luo, Xigun Yan, Qin Cui, Bin Xu, Huiying Xu, Zhiping Cai\*, Opt. Commu. 380(1), 357(2016)

[Red and orange Pr3+:LiYF4 planar waveguide laser]. Florent Starecki, Western Bolaños, Alain Braud, Jean-Louis Doualan, Gurvan Brasse, Abdelmjid Benayad, Virginie Nazabal, Bin Xu, Richard Moncorgé, and Patrice Camy, “Red and orange Pr3+:LiYF4 planar waveguide laser,” Opt. Lett. 38(4), 455(2013)

[Green, orange, and red Pr3+∶YLiF4 epitaxial waveguide lasers]. Western Bolaños, Gurvan Brasse, Florent Starecki, Alain Braud, Jean-Louis Doualan, Richard Moncorgé, and Patrice Camy, “Green, orange, and red Pr3+∶YLiF4 epitaxial waveguide lasers,” Opt. Lett. 39(15), 4450(2014)

[Blue Pr3+-doped ZBLAN fiber upconversion laser]. D. M. Baney, G. Rankin, and Kok-Wai Chang, “Blue Pr3+-doped ZBLAN fiber upconversion laser”, Opt. Lett. Vol. 21(17) 1372 (1996)

[Visible–NIR tunable Pr3+-doped fiber laser pumped by a GaN laser diode]. Hideyuki Okamoto, Ken Kasuga, Ikunari Hara, and Yoshinori Kubota, “Visible–NIR tunable Pr3+-doped fiber laser pumped by a GaN laser diode,” Opt. Express 17(22), 20227 (2009)

[High-power direct green laser oscillation of 598 mW in Pr3+-doped waterproof fluoroaluminate glass fiber excited by two-polarization-combined GaN laser diodes]. J. Nakanishi, Y. Horiuchi, T. Yamada, O. Ishii, M. Yamazaki, M. Yoshida, and Y. Fujimoto, “High-power direct green laser oscillation of 598 mW in Pr3+-doped waterproof fluoroaluminate glass fiber excited by two-polarization-combined GaN laser diodes,” Opt. Lett. 36, 1836–1838 (2011).

[Visible laser operation in a Pr3+:LiLuF4 monocrystalline fiber grown by the micro-pulling-down method]. Alberto Sottile, Zhonghan Zhang, Stefano Veronesi, Daniela Parisi, Alberto Di Lieto, and Mauro Tonelli, “Visible laser operation in a Pr3+:LiLuF4 monocrystalline fiber grown by the micro-pulling-down method,” Optical Materials Express 6(6) 1964-1972 (2016)

[Diode pumping of a continuous-wave Pr3+-doped LiYF4 laser]. A. Richter, E. Heumann, E. Osiac, G. Huber, W. Seelert, and A. Diening, “Diode pumping of a continuous-wave Pr3+-doped LiYF4 laser,” Opt. Lett. 29(22) 2638 (2004)

[Visible laser emission of solid state pumped LiLuF4:Pr3+]. F. Cornacchia, A. Richter, E. Heumann, G. Huber, D. Parisi, and M. Tonelli, “Visible laser emission of solid state pumped LiLuF4:Pr3+,” Opt. Express 15(3) 992 (2007)

[Diode pumped laser operation and spectroscopy of Pr3+:LaF3]. F. Reichert, F. Moglia, D.-T. Marzahl, P. Metz, M. Fechner, N.-O. Hansen, and G. Huber, “Diode pumped laser operation and spectroscopy of Pr3+:LaF3,” Opt. Express 20(18) 20387-20395 (2012)

[Wide wavelength tunability and green laser operation of diode-pumped Pr3+:KY3F10]. Philip W. Metz, Sebastian Müller, Fabian Reichert, Daniel-Timo Marzahl, Francesca Moglia, Christian Kränkel, and Günter Huber, “Wide wavelength tunability and green laser operation of diode-pumped Pr3+:KY3F10,” Opt. Express 21(25) 31274 (2013)

[Cr4+-Doped Y3Al5O12 as a Saturable Absorber for a Q-Switched and Mode-Locked 639-nm Pr3+-Doped LiYF4 Laser]. R. Abe, J. Kojou, K. Masuda, and F. Kannari, “Cr4+-Doped Y3Al5O12 as a Saturable Absorber for a Q-Switched and Mode-Locked 639-nm Pr3+-Doped LiYF4 Laser,” Appl. Phys. Express 6, 032703 (2013).

[InGaN diode pumped actively Q-switched intracavity frequency doubling Pr:LiYF4 261 nm laser]. J. Kojou, R. Abe, R. Kariyama, H. Tanaka, A. Sakurai, Y. Watanabe,

and F. Kannari, “InGaN diode pumped actively Q-switched intracavity frequency doubling Pr:LiYF4 261 nm laser,” Appl. Opt. 53, 2030 (2014).

[Passively Q-switched Pr:YLF laser]. S. V. Savitski, I. M. Ranieri, A. B. Krysa, and S. Calvez, “Passively Q-switched Pr:YLF laser,” in CLEO: Laser Applications to Photonic Applications, OSA Technical Digest (CD) (Optical Society of America, 2011), paper CMB7.

[Wavelength Tunable Q-switch Laser in Visible Region with Pr3+-doped Fluoride-glass Fiber Pumped by GaN Diode Lasers]. Fumihiko Kannari and Jyuichiro Kojyo, “Wavelength Tunable Q-switch Laser in Visible Region with Pr3+-doped Fluoride-glass Fiber Pumped by GaN Diode Lasers,” Conference on Lasers and Electro-Optics 2012, OSA Technical Digest (online) (Optical Society of America, 2012), paper JW2A.28.

[Intracavity second-harmonic generation at 320 nm of an actively Q-switched Pr:LiYF4 laser]. Junichiro Kojou, Yoichiro Watanabe, Yosuke Kojima, Hiroyuki Nemoto, and Fumihiko Kannari, “Intracavity second-harmonic generation at 320 nm of an actively Q-switched Pr:LiYF4 laser” Appl. Opt. 51(9) 1382-1386 (2012)

[InGaN diode pumped actively Q-switched intracavity frequency doubling Pr:LiYF4 261 nm laser]. J. Kojou, R. Abe, R. Kariyama, H. Tanaka, A. Sakurai, Y. Watanabe, and F. Kannari, “InGaN diode pumped actively Q-switched intracavity frequency doubling Pr:LiYF4 261 nm laser,” Appl. Opt. 53, 2030–2036 (2014).

[Saturation of 640-nm absorption in Cr4+:YAG for an InGaN laser diode pumped passively Q-switched Pr3+:YLF laser]. H. Tanaka, R. Kariyama, K. Iijima, K. Hirosawa, and F. Kannari,“Saturation of 640-nm absorption in Cr4+:YAG for an InGaN laser diode pumped passively Q-switched Pr3+:YLF laser,” Opt. Express 23, 19382–19395 (2015).

[50-kHz, 50-ns UV pulse generation by diode-pumped frequency doubling Pr3+:YLF Q-switch laser with a Cr4+:YAG saturable absorber]. Hiroki Tanaka, Ryosuke Kariyama, Kodai Iijima, and Fumihiko Kannari, “50-kHz, 50-ns UV pulse generation by diode-pumped frequency doubling Pr3+:YLF Q-switch laser with a Cr4+:YAG saturable absorber,” Appl. Opt. 55(23) 6193-6198 (2016)

[Gold nanoparticles as a saturable absorber for visible 635 nm Q-switched pulse generation]. D. Wu, J. Peng, Z. Cai, J. Weng, Z. Luo, N. Chen, and H. Xu, “Gold nanoparticles as a saturable absorber for visible 635 nm Q-switched pulse generation,” Opt. Express 23, 24071–24076 (2015).

[Atomic-layer molybdenum sulfide optical modulator for visible coherent light]. Y. Zhang, S. Wang, H. Yu, H. Zhang, Y. Chen, L. Mei, A. Di Lieto, M. Tonelli, and J. Wang, “Atomic-layer molybdenum sulfide optical modulator for visible coherent light,” Sci. Rep. 5, 11342 (2015).

[Passive Q-switching of a diode-pumped Pr:LiYF4 visible laser using WS2 as saturable absorber]. Y. Cheng, J. Peng, B. Xu, H. Yang, Z. Luo, H. Xu, Z. Cai, and J. Weng,“Passive Q-switching of a diode-pumped Pr:LiYF4 visible laser using WS2 as saturable absorber,” IEEE Photon. J. 8, 1–6 (2016).