Using laser diode as the pump source, an efficient self-mode-locked green and red visible laser with average output powers of more than 0.68 W and 1.44 W are demonstrated in this work, which are believed to be the highest average output power for mode locked lasers operating in visible wavelength region [1,2,3,4,5,6]. Moreover, Mechanism of the self-mode-locked Pr:YLF visible lasers is, for the first time, analyzed theoretically.

[1] S. Ruan, B. H. T. Chai, J. M. Sutherland, P. M. W. French, and J. R. Taylor, “Kerr-lens mode-locked visible transitions of a Pr:YLF laser,” Opt. Lett. **20**, 1041-1043 (1995).

[2] Y. P. Tong, A. V. Shestakov, B. H. T. Chai, J. M. Sutherland, P. M. W. French, and J. R. Taylor, “Self-starting Kerr-lens mode-locked femtosecond Cr4+:YAG and picosecond Pr3+:YLF solid-state lasers,” Opt. Lett. **21**, 644-646 (1996).

[3] M. Gaponenko, P. W. Metz, A. Härkönen, A. Heuer, T. Leinonen, M. Guina, T. Südmeyer, G. Huber, and C. Kränkel, “SESAM mode-locked red praseodymium laser,” Opt. Lett. **39**(24), 6939 (2014).

[4] Y. X. Zhang, H. H. Yu, H. J. Zhang, A. D. Lieto, M. R. Tonelli, and J. Y. Wang, “Laser-diode pumped self-mode-locked praseodymium visible lasers with multi-gigahertz repetition rate,” Opt. Lett. **41**(12), 2692(2016).

[5] Y. X. Zhang, H. H. Yu, R. Zhang, G. Zhao, H. J. Zhang, Y. X. Chen, L. M. Mei, M. R. Tonelli, and J. Y. Wang, “Broadband atomic-layer MoS2 optical modulators for ultrafast pulse generations in the visible range”. Opt. Lett. **42**(3), 547 (2017).

[6] K. Iijima, R. Kariyama, H. Tanaka, and F. Kannari, “Pr3+:YLF mode-locked laser at 640 nm directly pumped by InGaN-diode lasers,” Applied Optics **55**(28), 7782 (2016).